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EXAMEN DE PESO Y BALANCE
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1.- If an aircraft CG is found to be at 24 percent of MAC, that 24
    percent is an expression of
a-  the distance from the TEMAC.
b-  distance from the LEMAC.
c-  average distance from the LEMAC to the wing center of lift. 
d- distance from the CMAC. 

2.- The maximum weight of an aircraft is 
a- the empty weight plus crew, máximum fuel, cargo, and baggage.
b- empty weight plus crew, passengers, and fixed equipment.
c- empty weight plus useful load. 
d- empty weight only 

3.- What should be clearly indicated on the aircraft weighing
    form? 

    a.- Minimum allowable gross weight. 
    b.- Weight of unusable fuel. 
    c.- Weighing points. 
    d.- Maximum allowable gross weight. 

 4.- What type of measurement is used to designate the arm in
       weight and balance computation?

    a.- Distance. 
    b.- Weight. 
    c.- Weight x distance. 
    d.- Long. 

  5.-  When dealing with weight and balance of an aircraft, the
        term 'maximum weight' is interpreted to mean the máximum

a-  weight of the empty aircraft.
b-  weight of the useful load.
c-  authorized weight of the aircraft and its contents.


     d.- Maximum permissible weight of a loaded aircraft (passengers, crew,
           and cargo)  without fuel.

     6.-  Zero fuel weight 

a-  is the dry weight plus the weight of full crew, passengers, and cargo.
b- basic operating weight without crew, fuel, and cargo.
c- maximum permissible weight of aloaded aircraft (passengers, crew,and cargo) without fuel.
d- empty weight only 

      7.-If it is necessary to weigh an aircraft with full fuel tanks, all
          fuel weight must be subtracted from the scale reading(s) except
          minimum fuel. 

     a.-including unusable fuel. 
     b.-except unusable fuel.
     c.-maximum permissible weight of a loaded aircraft (passengers, crew,
         and cargo) 
     d.-without fuel.


      8.- Most modern aircraft are designed so that if all seats are
           occupied, full baggage weight is carried, and all fuel tanks
           are full, what will be the weight condition of the aircraft?

      a.-It will be in excess of máximum takeoff weight.
      b.-It will be at maximum basic
      c.-operating weight (BOW).

     9.- It will be at maximum taxi or ramp 

        a.-weight.
        b.- It will be at maximum landing
        c.- weight (BOW). 
     10.- Cuales son los documentos soporte para el programa de peso y
           balance de un Avion:

        a.- Manual del fabricante, practicas estándar, MGM
        b.- Certificado tipo, Manual de Mantenimiento, Manual de vuelo
        c.- Data sheft, Manual IPC, Manual del hangar
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