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1. The monocoque fuselaje rilies largery on the strenger of 

A. Longerons and formers. 
B. Skin and covering 
C. Bulheads and skin 
 
2. You can distinguish between aluminum and aluminum allow by 

A. Filing the metal 
B. Testing with an acetic acid solutio 
C. Testing with a 10 % solution of caustic soda. 
 
3. When straightening members made of 2024-T4, you should  

A. Straighten cold and Reinforce. 
B. Straighten cold and anneal to remove strees 
C. Apply heat to the inside of the bend. 
 
4. Aircraft structural units, such as spars, engine supports, Etc., which have been built 
       up from sheet metal, are normally 

A. Repairable, using approved methods. 
B. Repairable, except when subjected to compressive loads. 
C. Not repairable, but must be replaced when damage or deteriorated. 
 
5. The cantiléver wing uses 

A. External struts or wire bracing. 
B. No external bracing. 
C. The skin to carry most of the load to the wing butt. 
 
6. Clad aluminum alloys are used in aircraft because they
 
A. Can be heat treated much easier than the other. 
B. Are less subject to corrosión than uncoated aluminum alloys. 
C. Are stronger than unclad aluminum alloys 
 
 
7. Rivet gauge, or transversal pitch is the distance between the 

A. Center of rivets in adjacent rows. 
B. Center of adjacent rivets in the same rows. 
C. Heads of rivets in the same row. 
 
8. Rivets pitch is the distance between the 
 
A. Centers of the rivets in adjacent rows. 
B. Centers of adjacent rivets in the same row. 
C. Heads of rivets in the same row. 
 
9. The primary alloying agent of 2024-T3 is indicated  by the number
 
A. 2 
B. 20 
C. 24 
 
10. The dimensions of an MS20430AD4-8 rivet are 

A. 1/8 inch in diameter and 1/4 inch long. 
B. 1/8 inch in diameter and 1/2 inch long. 
C. 4/16 inch in diameter and 8/32 inch long. 
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