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EXAMEN DE OPERACIÓN EN TIERRA

NOMBRE ___________________________________________________
GRUPO  __________________                  FECHA___________________


	

                        1.-  The main differences between grades 100 and 100LL fuel are

	                               volatility and lead content. volatility, lead content, and color lead content and color

	.                              When towing a large aircraft:

	


	

	  A. - a person should be in the cockpit to watch for obstructions.

	  B. - persons should be stationed at the nose, each wingtip, and the empennage at all times.

	  C. - a person should be in the cockpit to operate the brakes. ...



	2.- When first starting to move an aircraft while taxiing, it is important to:


	   A.- test the brakes.....

	   B. - closely monitor the instruments.

	   C. - notify the control tower.



	  3.- Which statement(s) is/are true regarding tiedown of small aircraft?


	  1. Manila (hemp) rope has a tendency to stretch when it gets wet.

	  2. Nylon or dacron rope is preferred to manila rope.

	  3. The aircraft should be headed downwind in order to eliminate or minimize wing lift.

	   4. Leave the nosewheel or tailwheel unlocked.


	 A) 1, 2, 3, and 4.

	 B) 1 and 2.

	 C) 2......

	4.-Which of the following is the most satisfactory extinguishing agent for use on a carburetor or intake fire?


	A) Dry chemical.

	B) A fine, water mist.

	C) Carbon dioxide. .....




	

	5.-The color of 100LL fuel is


	A) blue.....

	B) colorless or straw.

	C) red.



	

	6.- When taxiing an airplane with a quartering tailwind, the elevators and

A. - upwind aileron should be held in the up position.

	B. - upwind aileron should be held in the down position.......

	C. - both ailerons should be kept in the neutral position.

	7. - What test is used to determine the serviceability of an oxygen cylinder?


	A. - Pressure test with manometer......

	B. - Pressure test with nitrogen.

	C. - Pressure test with water.






	  8.-A fire extinguisher container can be checked to determine its charge by


	  A. - attaching a remote pressure gauge.

	  B. - weighing the container and its contents......

	  C.- a hydrostatic test




    9. - The standard position for a signalman is slightly ahead of and in line with the aircraft's
          left wingtip

   A- True.....
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